
1.connect the serial port in the correct side of the broad. (with a white square around)  
 (Tekening Harvey Zhou)

2. telnet/serial port to the IPC, login with root/123456  
  
3. put command "resetconfig", and wait camera reboot

Deze kabel is benodigd voor de seriële verbinding:

